**TEST SCENARIO OF COFFEE VENDING MACHINE**

TS1: Verify that dimension of coffee machine is as per specification.

TS2: Verify that outer body and inner body materials are same as specified.

TS3: Verify the colour of the machine.

TS4: Verify the functioning of all button when it presses.

TS5: Check whether indicator lights are displaying correctly.

TS6: Verify the quantity of coffee poured in a single operation and ensure that no coffee is stored in the nozzle area.

TS7:Verify that coffee should not leak when not in operation.

TS8: Verify that machine is able to give balance by coin or by cash.

TS9:Verify that machine accepts all types of coins and cash.

TS10: Verify that how much coffee will get for a particular amount.

TS11: Verify that all buttons on the machine aligned as per requirement.

TS12: Ensure that all buttons have same functions as mentioned.

TS13:Verify that how much amount of coffee will get for particular amount of money.

TS14: Verify the mixing proportionality

TS15: Verify the time required to make coffee.

TS16:Check whether it have space to place cup.

TS17:Check whether it works in low voltage.

TS18:Check whether it automatically off after filling.

TS19:In case of touch check whether touch screen is working.

TS20:Verify that beep sound is working.

TS21: Check whether it is stable on surface.

TS22:Ensure that it do not have shock.

TS23:Verify that hole of the nozzle is enough sized.

TS24:Verify that machine should not take too much sound when operates.

TS25:Verify the amount of time machine takes to serve a single serving of coffee.

TS26: Verify that there is passage for extra coffee in machine.

TS27 :Ensure that cleaning mechanism works properly.

TS28:Check whether the machine displays error when runs out of ingredient.

TS29:Check whether temperature of coffee served should be same temperature or not.

TS30: Check whether input mechanism for coffee ingredients milk, water ,powder, sugar work as expected.

TS31: Verify that cancel option is working or not.

TS32:Check whether how coffee vending machine works when user press all button at once.

TS33: Verify that half cup facility is working properly.

TS34:Verify the working of machine when power supply is improper.

TS35:Ensure that sound of machine is not too noisy.

TS36:Verify that coffee is not dispensed when customer does not enter enough money , the money should be returned to customer.

TS37: Verify machine operation when one of ingredient is empty.